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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: CHINA
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
State Administration for Market Regulation (Standardization Administration of the P.R.C.)
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): Blowers (HS code(s): 8504); (ICS code(s): 29.180)

	5.
	Title, number of pages and language(s) of the notified document: National Standard of the P.R.C., Minimum allowable values of energy efficiency and energy efficiency grades for blowers; (21 page(s), in Chinese)

	6.
	Description of content: This document specifies the minimum allowable values of energy, energy efficiency levels, and test methods for turbine blowers and volumetric blowers.
This document applies to genera-purpose turbine blowers (including single-stage cantilever, single-stage double support, and multi-stage turbine blowers) with exhaust pressure (gauge pressure) ranging from 30 kPa to 200 kPa, or overall pressure ratio ranging from 1.3 to 3.0:
a) Mechanical supported centrifugal blower with an inlet flow rate of 500~1000000m3/h;
b) Axial flow blower with an inlet flow rate of 60000~10000000m3/h;
c) A suspended centrifugal blower with an import flow rate of 500~40000m3/h.
This document applies to single-stage Roots blowers with standard volumetric flow rates ranging from 1 to 1250m3/min, including positive pressure Roots blowers with pressure increases of 9.8 to 98kPa and negative pressure Roots blowers with pressure increases of 9.8 to 49kPa.
This document applies to screw blowers (including general purpose oil injected/oil-free single/twin screws) with a standard volumetric flow rate of 2 to 200m3/min and a pressure increase of 39.2 to 245kPa.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of the environment; Cost saving and productivity enhancement

	8.
	Relevant documents: 
-

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: To be determined 12 months after approval

	10.
	Final date for comments: 60 days from notification

	11.
	Texts available from: National enquiry point [X] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
WTO/TBT National Notification and Enquiry Center of the People's Republic of China
Tel：+86 10 57954633 / 57954627
E_mail: tbt@customs.gov.cn
https://members.wto.org/crnattachments/2025/TBT/CHN/25_03003_00_x.pdf
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