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NOTIFICATION
Addendum
The following communication, dated 3 June 2025, is being circulated at the request of the delegation of the State of Kuwait.

_______________


Title: "Rotating electrical machines - Efficiency classes of AC operated motors"
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Description: KWS 1897 specifies efficiency classes for single-speed electric motors that are rated according to IEC 60034-1 and rated for operation on a sinusoidal voltage supply. The scope of the standard, as well as its exceptions, is defined in the following Table 1.
Table 1: General Motors covered in KWS 1897 standards
	Number of poles
	2, 4, 6, 8

	Power range
	0.12 – 375 kW

	Number of phases
	3 Phase only

	Efficiency Level
	IE1 - Standard Efficiency
IE2 - High Efficiency
IE3 - Premium Efficiency
IE4 - Super Premium Efficiency

	Voltage
	< 1000 V, 50 Hz

	Degree of protection
	All

	Operating mode
	S1 (permanent operation with constant load); motors, that are designed for different operating modes but can still be operated permanently with rated output.

	Degree of temperature
	-20°C - +60°C

	Altitude
	Up to 4000 m above sea level

	Geared motors
	Included

	Smoke Extraction Motors with a temperature class up to 400°C
	Included
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