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NOTIFICATION
Addendum
The following communication, dated 1 July 2025, is being circulated at the request of the delegation of the State of Kuwait.

_______________


Title: Electrical accessories - Cable reels for household and similar purposes
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Description: Replace the whole text of this clause by the following: 
This International Standard applies to cable reels for a.c. only, with a rated voltage above
50 V and not exceeding 250 V for single-phase cable reels and above 50 V and not exceeding
440 V for all other cable reels, and a rated current not exceeding 16 A. They are intended for
household, commercial and light industrial and similar purposes, either indoors or outdoors,
with particular reference to safety in normal use.
This standard does not apply to:
– cable reeling devices incorporated in appliances or luminaires;
– cable reeling devices associated with appliances or luminaires.
NOTE 1 Requirements for cable reeling devices incorporated in appliances are specified in IEC 60335-1 and
IEC 60335-2-2.
NOTE 2 Requirements for cable reeling devices incorporated in luminaires are specified in IEC 60598-1 and
IEC 60598-2-25.
NOTE 3 A cable reeling device associated with an appliance or luminaire is a device designed to supply a specific
appliance or luminaire. It must be fixed to or delivered with the appliance or luminaire, without being incorporated
in it and having its own enclosure which provides protection against electric shock. An example is a cable reeling
device associated with handlamps according to IEC 60598-2-8.
This standard may be used as a guide for cable reeling devices incorporated or associated in
appliances or luminaires as far as it is applicable.
61242 Amend.1 © IEC:2008 – 3 –
Cable reels complying with this standard are suitable for use at ambient temperatures not
normally exceeding 25 °C, but occasionally reaching 35 °C.
In locations where special conditions prevail, special construction may be required.
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