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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: THE STATE OF KUWAIT
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
Public Authority for Industry
Standard and Metrology Department (KOWSMD)
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): Plugs and socket-outlets for household and similar purposes - Part 1: General requirements" (ICS 29.120.30) Plugs, socket-outlets, couplers

	5.
	Title, number of pages and language(s) of the notified document: Plugs and socket-outlets for household and similar purposes - Part 1: General requirements; (196 page(s), in English)

	6.
	Description of content:  IEC 60884-1:2022 applies to plugs and fixed or portable socket-outlets for AC only, with or without earthing contact, with a rated voltage greater than 50 V but not exceeding 440 V and a rated current not exceeding 32 A, intended for household and similar purposes, either indoors or outdoors.
Compatible plugs and socket-outlets, when combined, form a plug and socket-outlet system. Standardized systems used around the world are reported in IEC/TR 60083.
The rated current is limited to 16 A maximum for accessories provided with screwless-type terminals.
This fourth edition cancels and replaces the third edition published in 2002, Amendment 1:2006 and Amendment 2:2013. This edition constitutes a technical revision.
This edition includes the following significant technical changes with respect to the previous edition:
plugs and socket-outlets incorporating pilot lights;
crimped connections in accessories;
insulation piercing terminals (IPT);
accessories to be used with American Wire Gauge (AWG) cables;
accessories used in T° below −5 °C down to and including −45 °C;
accessories used in T° above +40 °C up to and including +70 °C;
plugs and socket-outlets for high load (HL);
clarification of some definitions;
durability of markings test;
introduction of thermal monitoring in the plug;
requirements for shutters in portable socket-outlets;
test walls for the verification of ingress of water;
rewriting of the temperature rise clause

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of human health or safety

	8.
	Relevant documents: 
[bookmark: _GoBack]GSO IEC 60884-1:2024

	9.
	Proposed date of adoption: 30 days from final date for comments
Proposed date of entry into force: 6 months from adoption

	10.
	Final date for comments: 30 August 2025，
[X] 60 days from notification

	11.
	Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
Public Authority for Industry
P.O.Box 4690, Safat
13047 Kuwait
Tel: (+965) 25302622
E-mail: Enquiry_point@pai.gov.kw
Website: http://www.pai.gov.kw/

https://members.wto.org/crnattachments/2025/TBT/KWT/25_04241_00_e.pdf
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