	[bookmark: bmkRestricted]
	

	[image: ]
	

	
	[bookmark: bmkSymbols]G/TBT/N/RWA/1234

	
	[bookmark: bmkDate][bookmark: spsDateDistribution]7 July 2025

	[bookmark: bmkSerial](25-4381)
	[bookmark: bmkTotPages]Page: 1/3

	[bookmark: bmkCommittee]Committee on Technical Barriers to Trade
	[bookmark: bmkLanguage][bookmark: spsOriginalLanguage]Original: English



tbtSymbol

- 1 -

[bookmark: spsSymbolHeader]G/TBT/N/RWA/1198

- 3 -

NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: RWANDA
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
Ministry of Trade and Industry (MINICOM), Republic of Rwanda
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): Road equipment and installations (ICS code(s): 93.080.30)

	5.
	Title, number of pages and language(s) of the notified document: DRS 607-4: 2025, Gully tops and manhole tops for vehicular and pedestrian areas — Specification — Part 4: Gully tops and manhole tops made of steel reinforced concrete.; (47 page(s), in English)

	6.
	Description of content:  This Draft Rwanda Standard specifies requirements, sampling and test methods for precast gully tops and manhole tops made of steel reinforced concrete with a clear opening up to and including 1 000 mm.
It is applicable to manhole tops and gully tops for use in areas subjected to pedestrian and/or vehicular traffic of class A 15, B 125, C 250, D 400, E 600 and F 900.
This Standard does not apply to:
— concave gratings for class D 400 installed in carriageways of roads or hard shoulders and concave gratings for classes F 900 and E 600;
— gratings/covers as part of prefabricated drainage channels;
— floor and roof gullies in buildings; and
— surface boxes.
NOTE This part 4 of DRS 607 is not applicable in isolation, but only in combination with DRS 607-1 and gives guidance for combinations of covers/gratings made of steel reinforced concrete with frames according to DRS 607-2, DRS 607-3, DRS 607-5 and DRS 607-6.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Consumer information, labelling; Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of the environment; Quality requirements; Reducing trade barriers and facilitating trade; Cost saving and productivity enhancement

	8.
	Relevant documents: 
1. DRS 607-1, Gully tops and manhole tops for vehicular and pedestrian areas — Part 1: Definitions, classification, general principles of design, performance requirements and test methods
2. DRS 607-2, Gully tops and manhole tops for vehicular and pedestrian areas — Part 2: Gully tops and manhole tops made of cast iron
3. DRS 607-3, Gully tops and manhole tops for vehicular and pedestrian areas — Part 3: Gully tops and manhole tops made of steel or aluminium alloys
4. DRS 607-5, Gully tops and manhole tops for vehicular and pedestrian areas — Part 5: Gully tops and manhole tops made of composite materials
5. DRS 607-6, Gully tops and manhole tops for vehicular and pedestrian areas — Part 6: Gully tops and manhole tops made of polypropylene (PP), polyethylene (PE) or unplasticized poly(vinyl chloride) (PVC-U)
6. RS 142, Design of concrete structures — General rules and rules for buildings — Code of
practice
7. RS 503, Precast concrete products — Performance requirements.RS ISO 1920-4, Testing of concrete — Part 4: Strength of hardened concrete
8. RS ISO 1920-4, Testing of concrete — Part 4: Strength of hardened concrete
9. RS ISO 22965-1, Part 1: Methods of specifying and guidance for the specifier.
10. RS ISO 22965-2, Concrete — Part 2: Specification of constituent materials, production of concrete and compliance of concrete.
11. [bookmark: _GoBack]RS ISO 1461, Hot dip galvanized coatings on fabricated iron and steel articles — Specifications and test methods

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 6 months from adoption

	10.
	Final date for comments: 5 September 2025，
[X] 60 days from notification 

	11.
	Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
Rwanda Standards Board (RSB)
KK 15 Rd, 49
P.O.BOX 7099, Kigali, Rwanda
Tel: +250 788303492
Email: info@rsb.gov.rw
Website: www.rsb.gov.rw 
https://members.wto.org/crnattachments/2025/TBT/RWA/25_04418_00_e.pdf
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