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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: RWANDA
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
Ministry of Trade and Industry (MINICOM), Republic of Rwanda
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): Road equipment and installations (ICS code(s): 93.080.30)

	5.
	Title, number of pages and language(s) of the notified document: DRS 607-5: 2025, Gully tops and manhole tops for vehicular and pedestrian areas — Specification — Part 5: Gully tops and manhole tops made of composite materials.; (47 page(s), in English)

	6.
	Description of content:  This Draft Rwanda Standard specifies requirements, sampling and test methods for gully tops and manhole tops made of composite materials with a clear opening up to and including 1 000 mm.
It is applicable to manhole tops and gully tops for use in areas subjected to pedestrian and/or vehicular traffic of class A 15, B 125, C 250 and D 400.
This Standard does not apply to:
⎯ manhole tops and gully tops manufactured by means of hand lay-up method;
⎯ gratings/covers as part of prefabricated drainage channels;
⎯ floor and roof gullies in buildings; and
⎯ surface boxes.
NOTE This Part 5 of DRS 607 is not applicable in isolation, but only in combination with DRS 607-1 and gives guidance for combinations of covers/gratings made of composite materials with frames according to DRS 607-2, DRS 607-3, DRS 607-4 or DRS 607-6.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Consumer information, labelling; Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of the environment; Quality requirements; Reducing trade barriers and facilitating trade; Cost saving and productivity enhancement

	8.
	Relevant documents: 
1. ASTM D2583-25, Standard Test Method for Indentation Hardness of Rigid Plastics by Means of a Barcol Impressor,
2. DRS 607-1, Gully tops and manhole tops for vehicular and pedestrian areas — Part 1: Definitions, classification, general principles of design, performance requirements and test methods
3. DRS 607-2, Gully tops and manhole tops for vehicular and pedestrian areas — Part 2: Gully tops and manhole tops made of cast iron
4. DRS 607-3, Gully tops and manhole tops for vehicular and pedestrian areas — Part 3: Gully tops and manhole tops made of steel or aluminium alloys
5. DRS 607-4, Gully tops and manhole tops for vehicular and pedestrian areas — Part 4: Gully tops and manhole tops made of steel reinforced concrete
6. DRS 607-6, Gully tops and manhole tops for vehicular and pedestrian areas — Part 6: Gully tops and manhole tops made of polypropylene (PP), polyethylene (PE) or unplasticized poly (vinyl chloride) (PVC-U)
7. RS ISO 868, Plastics and ebonite — Determination of indentation hardness by means of a durometer (Shore hardness)
8. RS 540, Reaction to fire tests for building products — Building products excluding floorings exposed to the thermal attack by a single burning item
9. RS 547, Fire classification of construction products and building elements — Classification using data from reaction to fire tests
10. ISO 62, Plastics — Determination of water absorption
11. ISO 175, Plastics — Methods of test for the determination of the effects of immersion in liquid chemicals
12. ISO 527-2, Plastics - Determination of tensile properties — Part 2: Test conditions for moulding and extrusion plastics
13. RS ISO 4892-2, Plastics — Methods of exposure to laboratory light sources — Part 2: Xenon-arc lamps
14. RS ISO 4892-3, Plastics — Methods of exposure to laboratory light sources — Part 3: Fluorescent UV lamps
15. ISO 1268-7, Fibre-reinforced plastics — Methods of producing test plates — Part 7: Resin transfer moulding
16. ISO 1268-8, Fibre-reinforced plastics — Methods of producing test plates — Part 8: Compression moulding of SMC and BMC
17. ISO 2878, Rubber, vulcanized or thermoplastic — Antistatic and conductive products — Determination of electrical resistance
18. [bookmark: _GoBack]ISO 3127, Thermoplastics pipes — Determination of resistance to external blows — Round-the-clock method

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 6 months from adoption

	10.
	Final date for comments: 5 September 2025，
[X] 60 days from notification 

	11.
	Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
Rwanda Standards Board (RSB)
KK 15 Rd, 49
P.O.BOX 7099, Kigali, Rwanda
Tel: +250 788303492
Email: info@rsb.gov.rw
Website: www.rsb.gov.rw 
https://members.wto.org/crnattachments/2025/TBT/RWA/25_04419_00_e.pdf
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