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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: CHINA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
State Administration for Market Regulation (Standardization Administration of the P.R.C.)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): LED products for indoor lighting (HS code(s): 853951; 940542); (ICS code(s): 27.010)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): National Standards of the P.R.C., Minimum allowable values of energy efficiency and energy efficiency grades of LED products for indoor lighting; (8 page(s), in Chinese)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2025/TBT/CHN/25_05370_00_x.pdf

	6.
	Description of content: This document specifies the energy efficiency grades, minimum allowable values of energy efficiency, and test methods for LED products for general indoor lighting, including LED downlights, directional integrated LED lamps, non-directional self-ballasted LED lamps, LED high bay luminaires, and double-capped LED lamps designed to retrofit liner fluorescent lamps.
This document applies to LED downlights, directional integrated LED lamps, non-directional self-ballasted LED lamps (including LED filament lamps), LED high bay luminaires, and double-capped LED lamps designed to retrofit liner fluorescent lamps, with a rated supply voltage not exceeding AC 250 V and a frequency of 50/60 Hz.
This document does not apply to non-directional self-ballasted LED lamps with additional optical lens designs, LED downlights and LED high bay luminaires using self-ballasted LED lamps, the LED products for indoor lighting with additional non-lighting related power-consuming functions or LED lighting products that are non-white or colour-tunable.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of the environment; Quality requirements

	8.
	Relevant documents: 
-

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: To be determined

	10.
	Provision of comments
Final date for comments: 20 October 2025
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
WTO/TBT National Notification and Enquiry Center of the People's Republic of China
Tel：+86 10 57954633/ 57954627
E_mail: tbt@customs.gov.cn
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