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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: DENMARK
If applicable, name of local government involved (Articles 3.2 and 7.2): Danish Road Traffic Authority
Sorsigvej 35
6760 Ribe
Denmark
Phone: +45 7221 8899
Email: info@fstyr.dk

	2.
	Agency responsible: 
Danish Road Traffic Authority
Sorsigvej 35
6760 Ribe
Denmark
Phone: +45 7221 8899
Email: info@fstyr.dk

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): VEHICLES OTHER THAN RAILWAY OR TRAMWAY ROLLING STOCK, AND PARTS AND ACCESSORIES THEREOF (HS code(s): 87)
Maximum permissible height and total weight of vehicles.

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): Order on the maximum width, length, height, weight and axle load of vehicles; (15 page(s), in Danish), (4 page(s), in Danish), (70 page(s), in Danish)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2025/TBT/DNK/25_05766_00_x.pdf
https://members.wto.org/crnattachments/2025/TBT/DNK/25_05766_01_x.pdf
https://members.wto.org/crnattachments/2025/TBT/DNK/25_05766_02_x.pdf

	6.
	Description of content: The Order on the maximum width, length, height, weight and axle load of vehicles sets the framework for vehicle dimensions and implements Council Directive 96/53/EC of 25 July 1996 establishing for certain road vehicles circulating within the EU the maximum authorised dimensions in national and international traffic and the maximum authorised weight in international traffic.
The draft order aims to ease a number of conditions covered by the order.
The draft order allows a maximum height for buses, lorries, tractors and motor equipment and their trailers of 4.20 m. Furthermore, the maximum permissible laden weight for vehicle combinations with seven or more axles is increased from 56 tonnes to 58 tonnes.
The police and military are also included in the provision on driving rescue boats. In addition, driving with an exceptionally wide snow plough is permitted on motorways.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: More lenient regulation than minimum requirements of Council Directive 96/53/EC.

	8.
	Relevant documents: 
The Danish Traffic Regulation Act (Færdselsloven)
Order on the maximum width, length, height, weight and axle load of vehicles (Bekendtgørelse om køretøjers største bredde, længde, højde, vægt og akseltryk)

	9.
	Proposed date of adoption: 1 December 2025
Proposed date of entry into force: 1 January 2026

	10.
	Provision of comments
Final date for comments: 31 October 2025
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
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