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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: TÜRKIYE
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Ministry of Industry and Technology
DG for EU and Foreign Affairs
Mustafa Kemal Mah. Dumlupinar Bulvari Eskişehir Yolu 2151. Cad. No:154 Cankaya - Ankara/ Türkiye
E-mail: sumeyye.sabanci@sanayi.gov.tr

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Ecodesign requirements for fans driven by motors with an electric input power between 125 W and 500 kW.

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): Draft Communiqué (2024/1834/EU) (SGM-2025/..) On Ecodesign Requirements For Fans Driven By Motors With An Electric Input Power Between 125 W and 500 kW; (18 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2025/TBT/TUR/25_06841_00_e.pdf

	6.
	Description of content: This Communiqué covers fans driven by motors with electrical input power between 125 W and 500 kW, including those integrated with other energy-related products specified in the Regulation on Eco-Design of Energy-Related Products
This Communiqué shall not apply to:
(a) fan impellers mounted on the shaft of electric motors with the sole purpose of cooling the motor itself;
(b) fans integrated into laundry and washer-dryers with maximum electric input power lower than or equal to 3 kW;
(c) fans integrated into kitchen hoods with total maximum electric input power attributable to the fan(s) lower than 280 W;
(d) fans with a best energy efficiency point at 8 000revolutions per minute or more;
(e) jet fans with maximum electric input power lower than 750 W;
3. This Communiqué shall not apply to fans that are specified to operate exclusively as follows and are specifically designed and marketed as such:
(a) in potentially explosive atmospheres, as defined in the Regulation on Equipment and Protective Systems Used in Potentially Explosive Atmosphere (2014/34/EU) published in the Official Gazette dated 30/6/2016 and numbered 29758
(b) for emergency use only, with regard to fire safety requirements as set out in the Construction Materials Regulation (305/2011/EU) published in the Official Gazette dated 10/7/2013 and numbered 28703, capable of short-time duty operation of 1 hour or more at temperatures of 300 °C and above;
(c) in nuclear installations; as defined in Regulation on Safety of Nuclear Facilities and Nuclear Materials
(d) in military establishments (bunkers) and civil defence establishments (bomb shelters);
(e) where operating temperatures of the gas being moved can be higher than 100 °C, or lower than – 40 °C, or both;
(f) where operating ambient air temperatures for the motor driving the fan, if located outside the gas stream, can be higher than 60 °C, or lower than – 30 °C, or both;
(g) with a supply voltage higher than 1 000V AC or higher than 1 500V DC;
(h) for handling toxic, highly corrosive or flammable gases or vapours;as defined in Regulation on Classification, Labeling, and Packaging of Substances and Mixtures
(i) for material transport, characterised by handling substances with a solid particle concentration of more than 10 mg/ m3 and particles with an average size of at least 0,1 mm and a hardness of at least 2 on the Mohs scale, while having an average blade angle of 50° to 90°;
(j) for handling gases containing biohazardous substances;
(k) for handling gases containing carcinogens or mutagens; as defined in Regulation on Health and Safety Measures in Work with Carcinogenic or Mutagenic Substances
(l) for handling gases with a compressibility factor, rounded to the nearest second decimal, in the designated pressure and temperature range of the scope that is not equal to 1,00;
(m) in cordless or battery-powered equipment;
(n) in handheld equipment whose weight is supported by hand during operation;
(o) in hand-guided mobile equipment moved while in operation;
(p) air circulating fans.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: The purpose of this Communiqué is to lay down ecodesign requirements for the placing on the market or putting into service of fans with an electric input power between 125 W and 500 kW (≥ 125 W and ≤ 500 kW) at their best efficiency point, including where they are integrated into other products for the implementation of the Regulation on Environmentally Responsible Design of Energy-Related Products put into force by the Presidential Decree No. 5187 dated 4/2/2022.
This Communiqué has been prepared within the framework of harmonization with European Union legislation based on Commission Regulation (EU) No 2024/1834 of July 3, 2024 on Eco-Design Requirements for Fans Driven by Motors with Electrical Input Power Between 125 W and 500 kW, Implementing Directive 2009/125/EC of the European Parliament and of the Council, Repealing Commission Regulation (EU) No 327/2011; Consumer information, labelling; Harmonization

	8.
	Relevant documents: 
Product Safety and Technical Regulations Law No. 7223 dated 5/3/2020, Article 388 of the Presidential Decree No. 1 on the Organization of the Presidency and the Regulation on Environmentally Responsible Design of Energy Related Products.
Commission Regulation (EU) No 2024/1834 of July 3, 2024 on Eco-Design Requirements for Fans Driven by Motors with Electrical Input Power Between 125 W and 500 kW, Implementing Directive 2009/125/EC of the European Parliament and of the Council, Repealing Commission Regulation (EU) No 327/2011

	9.
	Proposed date of adoption: This Communique will be adopted upon its publication.
Proposed date of entry into force: This Communique;
a) Article 8 and the second paragraph of Provisional Article 1 enters into foce on the date of publication,
b) Other provisions enter into force on 24/7/2027.

	10.
	Provision of comments
Final date for comments: 12 December 2025
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
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