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NOTIFICATION
Addendum
The following communication, dated 25 February 2026, is being circulated at the request of the delegation of the United States of America.

_______________


Title: Unlicensed Use of the 6 GHz Band; Expanding Flexible Use in Mid-Band Spectrum Between 3.7 and 24 GHz
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	Comment period changed - date: 
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	[bookmark: _Ref40866877]Text of final measure available from[footnoteRef:2]:  [2:  This information can be provided by including a website address, a pdf attachment, or other information on where the text of the final/modified measure and/or interpretive guidance can be obtained.] 

https://members.wto.org/crnattachments/2026/TBT/USA/final_measure/26_01144_00_e.pdf
https://members.wto.org/crnattachments/2026/TBT/USA/final_measure/26_01144_01_e.pdf

	[ ]
	Notified measure withdrawn or revoked - date: 
Relevant symbol if measure re-notified: 

	[ ]
	Content or scope of notified measure changed and text available from1: 
New deadline for comments (if applicable): 

	[ ]
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	Other: 



Description: In this document, the Federal Communications Commission (Commission or FCC) adopts rules allowing unlicensed geofenced variable power (GVP) devices to operate in the U-NII-5 and U-NII-7 portions of the 6 GHz band (5.925-7.125 GHz) at up to 11 dBm/MHz EIRP power spectral density and 24 dBm EIRP. GVP devices must use geofencing systems to prevent harmful interference to licensed microwave links and radio astronomy observatories. The geofencing systems will calculate exclusion zones where GVP devices cannot operate on specified frequencies. Each GVP access point must have a geolocation capability to determine its location and avoid operating on prohibited frequencies within the exclusion zones. Client devices must operate 6 dB below the access point's authorized power. These rules permit the GVP devices to operate at higher power than very lower power 6 GHz band unlicensed devices.
This rule is effective 27 April 2026.
91 Federal Register (FR) 9140, 25 February 2026; Title 47 Code of Federal Regulations (CFR) Parts 0 and 15:
https://www.govinfo.gov/content/pkg/FR-2026-02-25/html/2026-03744.htm
https://www.govinfo.gov/content/pkg/FR-2026-02-25/pdf/2026-03744.pdf
https://docs.fcc.gov/public/attachments/FCC-26-1A1.pdf
This final rule is identified by ET Docket No. 18-295 and GN Docket No. 17-183; FCC 26-1 and provide access to associated documents. The full text of the rule is available from the Commission's website at https://docs.fcc.gov/public/attachments/FCC-26-1A1.pdf. Documents are also accessible from the FCC's Electronic Document Management System (EDOCS) by searching the Docket Number. Filings (comments) are accessible at https://www.fcc.gov/ecfs/search/search-filings/results?q=(proceedings.name:(%2218-295%22)).
Comments on the proposed rule, notified as G/TBT/N/USA/1727/Rev.3, are due on or before 23 March 2026, and reply comments are due on or before 21 April 2026. WTO Members and their stakeholders are asked to submit comments to the USA TBT Enquiry Point by or before 4pm Eastern Time on 21 April 2026. Comments received by the USA TBT Enquiry Point from WTO Members and their stakeholders will be shared with the FCC and will also be submitted to the Electronic Comment Filing System (ECFS) if received within the comment period.
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