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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: CHINA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
State Administration for Market Regulation (Standardization Administration of the P.R.C.)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Motors (HS code(s): 8504); (ICS code(s): 27.010)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): National Standard of the P.R.C., Minimum allowable values of energy efficiency and energy efficiency grades for motors; (12 page(s), in Chinese)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/CHN/26_04311_00_x.pdf

	6.
	Description of content: This document specifies the energy efficiency grades, energy efficiency limit values, and test methods for three-phase asynchronous motors supplied by the power grid, variable-frequency speed-regulating three-phase asynchronous motors, single-phase asynchronous motors, and motors used for air conditioner fans.
This document applies to general-purpose motors or general-purpose explosion-proof motors with rated voltage below 1000V, powered by a 50Hz three-phase AC supply, rated power ranging from 120W to 1000kW, and with 2, 4, 6, or 8 poles, featuring a single-speed enclosed self-fan cooling design, N design, and continuous duty.
This document applies to general-purpose motors or general-purpose explosion-proof motors with rated voltage below 1000V, rated speed ranging from 600r/min to 6000r/min, powered by a frequency converter, rated power within the range of 120W to 1000kW, cooling method of IC416, and continuous duty.
This document also applies to general-purpose motors such as capacitor-start induction motors (120W~3700W), capacitor-run induction motors (120W~2200W), dual-capacitor induction motors (250W~3700W), as well as capacitor-run motors (10W~1100W) and brushless DC motors (10W~1100W) for air conditioner fans, all operated at voltage of 690V and below with 50Hz AC power supply.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of the environment; Cost saving and productivity enhancement

	8.
	Relevant documents: 
-

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 12 months after approval

	10.
	Provision of comments
Final date for comments: 18 October 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
WTO/TBT National Notification and Enquiry Center of the People's Republic of China
Tel：+86 10 57954633/ 57954642
E_mail: tbt@customs.gov.cn
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