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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: THE STATE OF KUWAIT
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Public Authority for Industry
Standard and Metrology Department (KOWSMD)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): All products fall under scope of " Switches for household and similar fixed electrical installations – Part 2-4: Particular requirements – Isolating switches " 

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): Switches for household and similar fixed electrical installations – Part 2-4: Particular requirements – Isolating switches; (37 page(s), in English), (37 page(s), in French)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/KWT/26_05237_00_e.pdf

	6.
	Description of content: Clause 1 of IEC 60669-1:2017 applies except as follows.
Replacement of the first paragraph with the following:
This part of IEC 60669 applies to manually operated general purpose isolating switches with a rated voltage not exceeding 440 V and a rated current not exceeding 125 A, intended for household and similar fixed electrical installations, either indoors or outdoors.
Replacement of the fifth dash of the third paragraph:
– a monophase circuit for motor load with a rated current up to 10 A and a power factor
not less than 0,6.
NOTE 101 Isolating switches are designed for overvoltage category III and used in environment of pollution degree 2 according to IEC 60664-1.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of human health or safety

	8.
	Relevant documents: 
GSO IEC 60669-2-4:2025 (Switches for household and similar fixed electrical installations - Part 2-4: Particular requirements - Isolating switches)

	9.
	Proposed date of adoption: 30 days from final date for comments.
Proposed date of entry into force: 1 year from adoption.

	10.
	Provision of comments
Final date for comments: 5 December 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Public Authority for Industry
P.O.Box 4690, Safat
13047 Kuwait
Tel: (+965) 25302622
E-mail: Enquiry_point@pai.gov.kw
Website: http://www.pai.gov.kw
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