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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: THE STATE OF KUWAIT
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Public Authority for Industry
Standard and Metrology Department (KOWSMD)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): All products fall under scope of " Switches for appliances - Part 2-1: Particular requirements for cord switches " 

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): Switches for appliances - Part 2-1: Particular requirements for cord switches;; (26 page(s), in English), (26 page(s), in French)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/KWT/26_05239_00_e.pdf

	6.
	Description of content: Clause 1 of IEC 61058-1:2016 is applicable except as follows:
Addition:
This document applies to cord switches (mechanical or electronic) for appliances actuated by hand, by foot or by other human activity, to operate or control electrical appliances and other equipment for household or similar purposes with a rated voltage not exceeding 250 V and a rated current not exceeding 16 A.
Throughout this document, the word "appliance" means "appliance or equipment".
These switches are intended to be operated by a person, via an actuating member or by actuating a sensing unit. The actuating member or sensing unit can be integral or arranged separately from the switch. The transmission of a signal between the actuating member or sensing unit and the switch can be made either physically or electrically (for example, electrical, optical, acoustic or thermal).
Switches which incorporate additional control functions governed by the switch function are within the scope of this document.
This document also covers the indirect actuation of the switch when the operation of the actuating member or sensing unit is provided by a remote control or a part of an appliance such as a door.
NOTE 1 Electronic switches can be combined with mechanical switches giving full disconnection or microdisconnection.
NOTE 2 Electronic switches without a mechanical switch in the supply circuit provide only electronic disconnection. Therefore, the circuit on the load side is always considered to be live.
NOTE 3 For switches used in tropical climates, additional requirements can apply.
NOTE 4 Attention is drawn to the fact that the standards for appliances can contain additional or alternative requirements for switches

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of human health or safety

	8.
	Relevant documents: 
GSO IEC 61058-2-1:2025 (Switches for appliances - Part 2-1: Particular requirements for cord switches)

	9.
	Proposed date of adoption: 30 days from final date for comments
Proposed date of entry into force: 1 year from adoption

	10.
	Provision of comments
Final date for comments: 6 December 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Public Authority for Industry
P.O.Box 4690, Safat
13047 Kuwait
Tel: (+965) 25302622
E-mail: Enquiry_point@pai.gov.kw
Website: http://www.pai.gov.kw
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