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NOTIFICATION
Addendum
The following communication, dated 8 January 2025, is being circulated at the request of the delegation of the United States of America.

_______________


Title: Anthropomorphic Test Devices, HIII 5th Percentile Female Test Dummy; Incorporation by Reference

	[bookmark: _Hlk24973414]Reason for Addendum:

	[ ]
	Comment period changed - date: 

	[ ]
	Notified measure adopted - date: 

	[X]
	Notified measure published - date: 3 January 2025

	[X]
	Notified measure enters into force - date: 18 February 2025; petitions for reconsideration for this final rule must be received no later than 18 February 2025.

	[X]
	[bookmark: _Ref40866877]Text of final measure available from[footnoteRef:1]:  [1:  This information can be provided by including a website address, a pdf attachment, or other information on where the text of the final/modified measure and/or interpretive guidance can be obtained.] 

The incorporation by reference of certain material listed in the rule is approved by the Director of the Federal Register as of 18 February 2025.
https://members.wto.org/crnattachments/2025/TBT/USA/final_measure/25_00315_00_e.pdf

	[ ]
	Notified measure withdrawn or revoked - date: 
Relevant symbol if measure re-notified: 

	[ ]
	Content or scope of notified measure changed and text available from1: 
New deadline for comments (if applicable): 

	[ ]
	Interpretive guidance issued and text available from1: 

	[ ]
	Other: 



Description: This document revises the chest jacket and spine box specifications for the Hybrid III 5th Percentile Female Test Dummy (HIII-5F). The jacket revisions resolve discrepancies between the jacket specifications in subpart O and jackets available in the field, and ensure a sufficiently low level of variation between jackets fabricated by different manufacturers. The spine box revisions eliminate a source of signal noise caused by fasteners within the box that may become loose during sled or vehicle crash tests. This rulemaking responds to a petition for rulemaking from the Alliance of Automobile Manufacturers.
Effective date: This rule is effective on 18 February 2025.
IBR date: The incorporation by reference of certain material listed in the rule is approved by the Director of the Federal Register as of 18 February 2025.
Petitions for reconsideration: Petitions for reconsideration for this final rule must be received no later than 18 February 2025.
90 Federal Register (FR) 250, 3 January 2025; Title 49 Code of Federal Regulations (CFR) Part 572:
https://www.govinfo.gov/content/pkg/FR-2025-01-03/html/2024-30985.htm
https://www.govinfo.gov/content/pkg/FR-2025-01-03/pdf/2024-30985.pdf
This final rule is identified by Docket Number NHTSA-2024-0093. The Docket Folder is available on Regulations.gov at https://www.regulations.gov/docket/NHTSA-2024-0093/document and provides access to primary and supporting documents. Documents are also accessible from Regulations.gov by searching the Docket Number. WTO Members and their stakeholders are asked to submit petitions for reconsideration for this final rule to the USA TBT Enquiry Point by or before 4pm Eastern Time on 18 February 2025. Petitions for reconsideration received by the USA TBT Enquiry Point from WTO Members and their stakeholders will be shared with NHTSA.
Previous actions notified under the symbol G/TBT/N/USA/1560 are identified by Docket Number NHTSA-2019-0023. The Docket Folder is available on Regulations.gov at https://www.regulations.gov/docket/NHTSA-2019-0023/document and provides access to primary and supporting documents as well as comments received. Documents are also accessible from Regulations.gov by searching the Docket Number.
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