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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: INDIA
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
Department for Promotion of Industry and Internal Trade (DPIIT)
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 
Shri Dheeraj Kumar Meena
Under Secretary to the Govt. of India
Department for Promotion of Industry and Internal Trade
Ministry of Commerce and Industry
Vanijya Bhawan, New Delhi
Telephone: +91-11-23038952
Email: lei-dpiit@gov.in , Dheeraj.meena17@gov.in
Website: https://dpiit.gov.in/

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): Chain Pulley Block, Ratchet Lever Hoist and Universal Gearless Pulling and Lifting Machine

	5.
	Title, number of pages and language(s) of the notified document: Chain Pulley Block, Ratchet Lever Hoist and Universal Gearless Pulling and Lifting Machine (Quality Control) Order, 2024; (2 page(s), in English)

	6.
	Description of content: Chain Pulley Block, Ratchet Lever Hoist and Universal Gearless Pulling and Lifting Machine (Quality Control) Order, 2025
Hand-operated chain pulley block: A Chain Pulley Block is a manual lifting device that uses a system of gears, chains, and hooks to lift and lower heavy objects. The block operates on a simple principle: applying force to the hand chain rotates internal gears, which amplify the force and move the load chain to lift the attached weight.
Ratchet Lever Hoist: It is a manual lifting device for raising and lowering heavy loads, where the main components typically include a lever, a chain or wire rope, a load hook, a brake, and a ratchet and pawl system.
Hand-Operated universal gearless pulling and lifting machines: The "Universe" gearless hand operated pulling and lifting machines are used for rectilinear pulling of steel wire ropes by the gripping and releasing actions of two sets of jaws alternately.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of the environment

	8.
	Relevant documents: 
To be published in the Gazette of India

	9.
	Proposed date of adoption: The date of notification in E-Gazette
Proposed date of entry into force: Six months from the date of notification in E-Gazette

	10.
	Final date for comments: 60 days from notification

	11.
	Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
Shri Dheeraj Kumar Meena
Under Secretary to the Govt. of India
Department for Promotion of Industry and Internal Trade
Ministry of Commerce and Industry
Vanijya Bhawan, New Delhi
Telephone: +91-11-23038952
Email: lei-dpiit@gov.in , Dheeraj.meena17@gov.in
Website: https://dpiit.gov.in/
https://members.wto.org/crnattachments/2025/TBT/IND/25_03510_00_e.pdf
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