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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: THE STATE OF KUWAIT
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
Public Authority for Industry
Standard and Metrology Department (KOWSMD)
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): All products fall under scope of " Water Heaters – Energy Performance Requirements and Labelling " (ICS 91.140.65) Water heating equipment 

	5.
	Title, number of pages and language(s) of the notified document: Water Heaters – Energy Performance Requirements and Labelling; (49 page(s), in English)

	6.
	Description of content:  This Kuwait Technical Regulation specifies the Minimum Energy Performance Standard (MEPS) and testing requirements of water heaters. 
Category of water heaters falling in the scope of this standard are
• Electric storage water heaters
• Instantaneous electric water heaters
• Heat pump water heaters
• Storage tanks
It shall apply to water heaters that operate in AC single-phase circuits of 240V or designed for dual voltage or voltage range including these values, and three-phase circuits of 415 V with a frequency of 50 Hz according to GSO 1899.
It shall apply to water heaters with power under or equal to 70 kW.
It shall apply to products with a capacity up to 2,000 liters for all types of water heaters except for gas fired water heaters where the maximum capacity is 300 liters.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Energy saving

	8.
	Relevant documents: 
N/A

	9.
	Proposed date of adoption: 30 days from final date for comments
Proposed date of entry into force: 1 year from adoption.

	10.
	Final date for comments: 5 September 2025，
[X] 60 days from notification

	11.
	Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
Public Authority for Industry (PAI)
P.O.Box:4690 Safat
13047 Kuwait
[bookmark: _GoBack]Tel.:(+965) 25302622
E-mail: Enquiry_point@pai.gov.kw
Website: http://www.pai.gov.kw

https://members.wto.org/crnattachments/2025/TBT/KWT/25_04471_00_e.pdf
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