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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: THE STATE OF KUWAIT
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
Public Authority for Industry (PAI)
Kuwait Standard & Metrology Department (KOWSMD)
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): All products fall under scope of Ceramic tiles (ICS code(s): 91.100.23) Construction materials and building (Vocabularies); (ICS code(s): 01.040.91)

	5.
	Title, number of pages and language(s) of the notified document: Ceramic tiles — Definitions, classification, characteristics and marking; (59 page(s), in English)

	6.
	Description of content:  This document defines terms and establishes classifications, characteristics and marking requirements for ceramic tiles of the best commercial quality (first quality). This document is not applicable to tiles made by other than normal processes of extrusion or dry pressing. It is not applicable to decorative accessories or trim such as edges, corners, skirting, capping, coves, beads, steps, curved tiles and other accessory pieces or mosaics (i.e. any piece that can fit into a square, the side of which is less than 7 cm).
NOTE ISO 10545 (all parts) describes the test procedures required to determine the product characteristics listed in this document. ISO 10545 is a multi-part standard, each part describes a specific test procedure or related matter.
plugs and socket-outlets for high load (HL);
clarification of some definitions;
durability of markings test;
introduction of thermal monitoring in the plug;
requirements for shutters in portable socket-outlets;
test walls for the verification of ingress of water;
rewriting of the temperature rise clause

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of the environment

	8.
	Relevant documents: 
GSO ISO 13006:2021 (Ceramic tiles — Definitions, classification, characteristics and marking)

	9.
	Proposed date of adoption: 30 days from final date for comments
Proposed date of entry into force: 6 months from adoption

	10.
	Final date for comments: 5 September 2025，
[X] 60 days from notification

	11.
	Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
Public Authority for Industry (PAI)
P.O.Box:4690 Safat
13047 Kuwait
Tel.:(+965) 25302622
E-mail: Enquiry_point@pai.gov.kw
Website: http://www.pai.gov.kw
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