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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: RWANDA
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
Ministry of Trade and Industry (MINICOM), Republic of Rwanda
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): Road equipment and installations (ICS code(s): 93.080.30)

	5.
	Title, number of pages and language(s) of the notified document: DRS 607-1:2025, Gully tops and manhole tops for vehicular and pedestrian areas — Specification — Part 1: Classification, general design and performance requirements.; (47 page(s), in English)

	6.
	Description of content: This Draft Rwanda Standard specifies classification, general design, performance requirements and test methods for gully tops and manhole tops.
It applies for manhole tops and gully tops with a clear opening up to and including 1 000 mm for installation within areas subjected to pedestrian and/or vehicular traffic.
This standard is not applicable to gratings as part of prefabricated drainage channels, floor and roof gullies in buildings and surface boxes.
NOTE This Part 1 of DRS 607 is not applicable in isolation, but only in combination with DRS 607-2, DRS 607-3, DRS 607-4, DRS 607-5 and DRS 607-6.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Consumer information, labelling; Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of the environment; Quality requirements; Reducing trade barriers and facilitating trade; Cost saving and productivity enhancement

	8.
	Relevant documents: 
1. RS ISO 868, Plastics and ebonite — Determination of indentation hardness by means of a durometer (Shore hardness)
2. RS ISO 7500-1, Metallic materials — Verification of static uniaxial testing machines — Part 1: Tension/compression testing machines— Verification and calibration of the force-measuring system
3. RS ISO 22965-1, Concrete — Part 1: Methods of specifying and guidance for the specifier
4. RS ISO 22965-2, Concrete — Part 2: Specification of constituent materials, production of concrete and compliance of concrete
5. RS 542, Determination of slip resistance of pedestrian surfaces — Methods of evaluation

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 6 months from adoption

	10.
	Final date for comments: 5 September 2025，
[bookmark: _GoBack][X] 60 days from notification 

	11.
	Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
Rwanda Standards Board (RSB)
KK 15 Rd, 49
P.O.BOX 7099, Kigali, Rwanda
Tel: +250 788303492
Email: info@rsb.gov.rw
Website: www.rsb.gov.rw 

https://members.wto.org/crnattachments/2025/TBT/RWA/25_04415_00_e.pdf
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