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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: RWANDA
If applicable, name of local government involved (Article 3.2 and 7.2): 

	2.
	Agency responsible: 
Ministry of Trade and Industry (MINICOM), Republic of Rwanda
Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above: 

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other: 

	4.
	Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable): Road equipment and installations (ICS code(s): 93.080.30)

	5.
	Title, number of pages and language(s) of the notified document: DRS 607-6: 2025, Gully tops and manhole tops for vehicular and pedestrian areas — Specification — Part 6: Gully tops and manhole tops made
of polypropylene (PP), polyethylene (PE) or unplasticized poly (vinyl chloride) (PVCU).; (47 page(s), in English)


	6.
	Description of content:   This Draft Rwanda Standard specifies requirements, sampling and test methods for manhole tops and gully tops made of Polypropylene, Polyethylene or unplasticized poly (vinyl chloride) by a moulding or extrusion process, with a clear opening up to and including 1 000 mm.
It is applicable to manhole tops and gully tops for use in areas subjected to pedestrian and/or vehicular traffic of class A 15 and B 125.
This Standard does not apply to:
⎯ rodding point covers;
⎯ gratings/covers as part of prefabricated drainage channels;
⎯ floor and roof gullies in; and
⎯ surface boxes.
NOTE This Part 6 of DRS 607 is not applicable in isolation, but only in combination with DRS 607-1 and gives guidance for combinations of covers/grating made of PP, PE or PVC–U with frames according to DRS 607-2, DRS 607 -3, DRS 607 -4 and DRS 607 -5.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Consumer information, labelling; Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of the environment; Quality requirements; Reducing trade barriers and facilitating trade; Cost saving and productivity enhancement

	8.
	Relevant documents: 
1. DRS 607-1, Gully tops and manhole tops for vehicular and pedestrian areas — Part 1: Definitions, classification, general principles of design, performance requirements and test methods
2. DRS 607-2, Gully tops and manhole tops for vehicular and pedestrian areas — Part 2: Gully tops and manhole tops made of cast iron
3. DRS 607-3, Gully tops and manhole tops for vehicular and pedestrian areas — Part 3: Gully tops and manhole tops made of steel or aluminium alloys
4. DRS 607-4, Gully tops and manhole tops for vehicular and pedestrian areas — Part 4: Gully tops and manhole tops made of steel reinforced concrete
5. DRS 607-5, Gully tops and manhole tops for vehicular and pedestrian areas — Part 5: Gully tops and manhole tops made of composite materials
6. ISO 8773, Plastics piping systems for non-pressure underground drainage and sewerage — Polypropylene (PP)
7. ISO 4435, Plastics piping systems for non-pressure underground drainage and sewerage — Unplasticized poly (vinyl chloride) (PVC-U)
8. ISO 8772, Plastics piping systems for non-pressure underground drainage and sewerage — Polyethylene (PE)
9. ISO 21138-1, Plastics piping systems for non-pressure underground drainage and sewerage — Structured-wall piping systems of unplasticized poly (vinyl chloride) (PVC-U), polypropylene (PP) and polyethylene (PE) Part 1: Material specification and performance criteria for pipes, fittings and systems
10. ISO 21138-2, Plastics piping systems for non-pressure underground drainage and sewerage — Structured-wall piping systems of unplasticized poly (vinyl chloride) (PVC-U), polypropylene (PP) and polyethylene (PE) — Part 2: Specifications for pipes and fittings with smooth internal and external surface and the system, Type A
11. ISO 21138-3, Plastics piping systems for non-pressure underground drainage and sewerage — Structured-wall piping systems of unplasticized poly (vinyl chloride) (PVC-U), polypropylene (PP) and polyethylene (PE) — Part 3: Specifications for pipes and fittings with smooth internal and profiled external surface and the system, Type B
12. RS 547, Fire classification of construction products and building elements — Classification using data from reaction to fire tests
13. ISO 13272, Plastics piping systems for non-pressure underground drainage and sewerage — Unplasticized poly (vinyl chloride) (PVC-U), polypropylene (PP), polypropylene with mineral modifiers (PP-MD) and polyethylene (PE) — Specifications for manholes and inspection chambers in traffic areas and underground installations.
14. RS 540, Reaction to fire tests for building products — Building products excluding floorings exposed to the thermal attack by a single burning item
15. D578/D578M-23, Standard Specification for Glass Fiber Strands
16. RS ISO 105-A03, Textiles — Tests for colour fastness Part A03: Grey scale for assessing staining
17. ISO 580:2005, Plastics piping and ducting systems — Injection-moulded thermoplastics fittings — Methods for visually assessing the effects of heating
18. ISO 1133-1, Plastics — Determination of the melt mass-flow rate (MFR) and melt volume-flow rate (MVR) of thermoplastics — Part 1: Standard method
19. ISO 1183-1, Plastics — Methods for determining the density of non-cellular plastics — Part 1: Immersion method, liquid pyknometer method and titration method
20. ISO 1183-2, Plastics — Methods for determining the density of non-cellular plastics — Part 2: Density gradient column method
21. ISO 3126, Plastics piping systems — Plastics components — Determination of d
22. ISO 4892-1, Plastics — Methods of exposure to laboratory light sources — Part 1: General guidance
23. ISO 4892-2, Plastics — Methods of exposure to laboratory light sources — Part 2: Xenon-arc lamps
24. ISO 4892-3, Plastics — Methods of exposure to laboratory light sources — Part 3: Fluorescent UV lamps
25. RS ISO 8256, Plastics — Determination of tensile-impact strength
26. ISO 9163, Textile glass — Rovings — Manufacture of test specimens and determination of tensile strength of impregnated rovings
27. ISO 178, Plastics — Determination of flexural properties
28. ISO 527-1, Plastics — Determination of tensile properties — Part 1: General principles
29. ISO 1888, Textile glass — Staple fibres or filaments — Determination of average diameter
30. ISO 3127, Thermoplastics pipes — Determination of resistance to external blows — Round-the-clock method
31. RS ISO 3506-1, Mechanical properties of corrosion-resistant stainless steel fasteners — Part 1: Bolts, screws and studs
32. RS ISO 3506-2, Mechanical properties of corrosion-resistant stainless-steel fasteners — Part 2: Nuts
33. ISO 6964, Polyolefin pipes and fittings — Determination of carbon black content by calcination and pyrolysis — Test method and basic specification
34. [bookmark: _GoBack]ISO 15100, Plastics — Reinforcement fibres — Chopped strands — Determination of bulk density

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 6 months from adoption

	10.
	Final date for comments: 5 September 2025，
[X] 60 days from notification 

	11.
	Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body: 
Rwanda Standards Board (RSB)
KK 15 Rd, 49
P.O.BOX 7099, Kigali, Rwanda
Tel: +250 788303492
Email: info@rsb.gov.rw
Website: www.rsb.gov.rw 

https://members.wto.org/crnattachments/2025/TBT/RWA/25_04420_00_e.pdf
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