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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: DENMARK
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Danish Road Traffic Authority
Sorsigvej 35 6760 Ribe Denmark Phone: +45 7221 8899 Email: info@fstyr.dk

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Motor vehicles for the transport of goods, incl. chassis with engine and cab (HS code(s): 8704)
The following four types of longer combination vehicles (EMS1, max. Length 25,25m):
1. Rigid truck, dolly, and semi-trailer
2. Truck/tractor unit, semi-trailer, and centre axle trailer
3. Truck/tractor unit, link-trailer, and semi-trailer
4. Rigid truck and drawbar trailer, that leads to a train length larger than 18.75 meters – 20.75 meters if the vehicle has a mounted crane with a capacity larger than 8 tm.

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): The Order on trial with vehicles in longer combination vehicles (EMS1, max. lenght 25,25 m) (Bekendtgørelse om køretøjer i forsøg med modulvogntog); (74 page(s), in Danish), (7 page(s), in Danish)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2025/TBT/DNK/25_05799_00_x.pdf
https://members.wto.org/crnattachments/2025/TBT/DNK/25_05799_01_x.pdf

	6.
	Description of content: The Order on trial with vehicles in longer combination vehicles (EMS1, max. lenght 25,25 m) sets the framework for the Danish trial with vehicles in longer combination vehicles.
The draft order aims to increase the weight limit on longer combination vehicles, and sets requirements for a certain percentage of the road train weight on the driving wheels when starting from a standstill when above a certain weight threshold
Furthermore, the length of longer combination vehicles can be extended if the extension is caused by an extended driver's cab.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of the environment; Harmonization; Reducing trade barriers and facilitating trade; Cost saving and productivity enhancement

	8.
	Relevant documents: 
The Danish Traffic Regulation Act (Færdselsloven)
The Order on trial with vehicles in longer combination vehicles (EMS1, max. lenght 25,25 m) (Bekendtgørelse om køretøjer i forsøg med modulvogntog)

	9.
	Proposed date of adoption: 3 December 2025
Proposed date of entry into force: 1 January 2026

	10.
	Provision of comments
Final date for comments: 1 November 2025
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Danish Business Authority
Langelinie Allé 17 DK-2100 Copenhagen O Denmark Phone: +45 35 29 10 00 E-mail: notifikationer@erst.dk
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