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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: MALAWI
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Malawi Bureau of Standards

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Fittings, e.g. joints, elbows, flanges, of plastics, for tubes, pipes and hoses (HS code(s): 391740); Plastics pipes (ICS code(s): 23.040.20)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): DMS 5:2022 Unplasticized polyvinyl chloride (UPVC) pipes and pipe fittings for use above ground in drainage installations – Specification; (5 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2025/TBT/MWI/25_07594_00_e.pdf
Director General
Malawi Bureau of Standards
P.O Box 946
Blantyre, Malawi
Tel: + 265 887376 444
Fax: + 265 1870 756
E-mail: info@mbsmw.org

	6.
	Description of content: This draft standard covers unplasticized poly(vinyl chloride) (PVC-U) pipes (including vent pipes and pipe fittings of nominal sizes 40 mm to 160 mm intended for above-ground non-pressure applications for the conveyance of soil (human excrement or faeces) and waste water where continuous temperatures in excess of 60 °C are not encountered.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Consumer information, labelling; Prevention of deceptive practices and consumer protection; Quality requirements; Reducing trade barriers and facilitating trade

	8.
	Relevant documents: 
1. ISO 4892-3, Plastics – Methods of exposure to laboratory light sources – Part 3: Fluorescent UV lamps.
2. SANS 527-2/ISO 527-1, Plastics – Determination of tensile properties – Part 2: Test conditions for moulding and extrusion plastics.
3. DMS 458/ISO 4633, Rubber seals – Joint rings for water supply, drainage and sewerage pipelines – Specification for materials.
4. SANS 9852/ISO 9852, Unplasticized poly(vinyl chloride) (PVC-U) – Dichloromethane resistance at specified temperature (DCMT) – Test method.
5. SANS 50681-1/EN 681-1, Elastomeric seals – Material requirements for pipe joint seals used in water and drainage applications – Part 1: Vulcanized rubber.

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: To be determined

	10.
	Provision of comments
Final date for comments: 6 January 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Director General
Malawi Bureau of Standards
P.O Box 946
Blantyre, Malawi
Tel: + 265 887376 444
Fax: + 265 1870 756
E-mail: info@mbsmw.org
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