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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: BURUNDI, KENYA, RWANDA, TANZANIA, UGANDA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Tanzania Bureau of Standards
Ubungo, Morogoro Road/Sam Nujoma Road
P. O. Box 9524
DAR ES SALAAM, TANZANIA
T el. No: +255 22 245 0298/+255 22 245 020
Telefax: +255 22 2450959,
Email: nep@tbs.go.tz
Website: www.tbs.go.tz 
E-mail: info@tbs.go.tz

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Petroleum oils and oils obtained from bituminous minerals (other than crude) and preparations n.e.s. or included, containing by weight 70 % or more of petroleum oils or of oils obtained from bituminous minerals, these oils being the basic constituents of the preparations, containing biodiesel (excl. waste oils) (HS code(s): 271020); Liquid fuels (ICS code(s): 75.160.20)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): DEAS 1301: 2025, Gasohol E5 and E10— Specification, First Edition; (16 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2025/TBT/TZA/25_08094_00_e.pdf
Tanzania Bureau of Standards
Ubungo, Morogoro Road/Sam Nujoma Road
P. O. Box 9524
DAR ES SALAAM, TANZANIA
T el. No: +255 22 245 0298/+255 22 245 020
Telefax: +255 22 2450959,
Email: nep@tbs.go.tz
Website: www.tbs.go.tz 
E-mail: info@tbs.go.tz

	6.
	Description of content: This draft East African Standard prescribes the requirements, test methods and sampling, method for gasohol E5 and E10 used as fuel in spark ignition engines

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Consumer information, labelling; Prevention of deceptive practices and consumer protection; Quality requirements; Harmonization; Reducing trade barriers and facilitating trade

	8.
	Relevant documents: 
1. ASTM D1298, Standard Test Method for Density, Relative Density, or API Gravity of Crude Petroleum and Liquid Petroleum Products by Hydrometer Method
2. ASTM D4052, Test Method for Density, Relative Density, and API Gravity of Liquids by Digital Density Meter
3. ASTM D86, Standard Test Method for Distillation of Petroleum Products and Liquid Fuels at Atmospheric Pressure
4. ISO 3675, Crude petroleum and liquid petroleum products — Laboratory determination of density — Hydrometer method
5. IP 123, Petroleum products — Determination of distillation characteristics at atmospheric pressure
6. ISO 2160, Petroleum products — Corrosiveness to copper — Copper strip test
7. IP154, Petroleum products — Corrosiveness to copper — Copper strip test
8. ASTM D130, Standard Test Method for Corrosiveness to Copper from Petroleum Products by Copper Strip Test
9. ASTM D4294, Standard Test Method for Sulfur in Petroleum and Petroleum Products by Energy Dispersive X-ray Fluorescence Spectrometry
10. ASTM D381, Standard Test Method for Gum Content in Fuels by Jet Evaporation
11. ASTM D4952, Standard Test Method for Qualitative Analysis for Active Sulfur Species in Fuels and Solvents (Doctor Test)
12. ASTM D3227, Standard Test Method for (Thiol Mercaptan) Sulfur in Gasoline, Kerosine, Aviation Turbine, and Distillate Fuels (Potentiometric Method)
13. ASTM D3237, Standard Test Method for Lead in Gasoline by Atomic Absorption Spectroscopy
14. IP 428, Liquid petroleum products — Petrol — Determination of low lead concentrations by atomic absorption spectrometry
15. IP429, Liquid petroleum products — Petrol — Determination of the benzene content by infrared spectrometry
16. ASTM D5580, Standard Test Method for Determination of Benzene, Toluene, Ethylbenzene, p/m-Xylene, o-Xylene, C9 and Heavier Aromatics, and Total Aromatics in Finished Gasoline by Gas Chromatography
17. ISO 5164, Petroleum products — Determination of knock characteristics of motor fuels — Research method
18. ASTM D2699, Standard Test Method for Research Octane Number of Spark-Ignition Engine Fuel
19. ASTM D323, Standard Test Method for Vapor Pressure of Petroleum Products (Reid Method)
20. ASTM D5191, Standard Test Method for Vapor Pressure of Petroleum Products and Liquid Fuels (Mini Method)
21. ISO 3007, Petroleum products and crude petroleum — Determination of vapour pressure — Reid method
22. ASTM D4815, Standard Test Method for Determination of MTBE, ETBE, TAME, DIPE, tertiary-Amyl Alcohol and C1 to C4 Alcohols in Gasoline by Gas Chromatography
23. ISO 22854, Liquid petroleum products — Determination of hydrocarbon types and oxygenates in automotive-motor gasoline and in ethanol (E85) automotive fuel — Multidimensional gas chromatography method
24. IP 40, Petroleum products — Determination of oxidation stability of gasoline — Induction period method
25. ISO 7536:1994, Petroleum products — Determination of oxidation stability of gasoline — Induction period method
26. ASTM D525, Standard Test Method for Oxidation Stability of Gasoline (Induction Period Method)
27. ISO 20847, Petroleum products — Determination of sulphur content of automotive fuels — Energy-dispersive
28. X-ray fluorescence spectrometry
29. ASTM D323, Standard Test Method for Vapor Pressure of Petroleum Products (Reid Method)
30. ASTM D5191, Standard Test Method for Vapor Pressure of Petroleum Products and Liquid Fuels (Mini Method)
31. EN 13016-1, Liquid petroleum products — Vapour pressure — Part 1: Determination of air saturated vapour pressure (ASVP) and calculated dry vapour pressure equivalent (DVPE)
32. ASTM D5453, Standard Test Method for Determination of Total Sulfur in Light Hydrocarbons, Spark Ignition Engine Fuel, Diesel Engine Fuel, and Engine Oil by Ultraviolet Fluorescence
33. ASTM D5580-21, Standard Test Method for Determination of Benzene, Toluene, Ethylbenzene, p/m-Xylene, o-Xylene, C9 and Heavier Aromatics, and Total Aromatics in Finished Gasoline by Gas Chromatography
34. ASTM D5599, Standard Test Method for Determination of Oxygenates in Gasoline by Gas Chromatography and Oxygen Selective Flame Ionization Detection
35. ISO 20847, Petroleum products — Determination of sulphur content of automotive fuels — Energy-dispersive
36. X-ray fluorescence spectrometry
37. KS 515: 2010, Gasohol 10 % (v/v) — Specification

	9.
	Proposed date of adoption: To be determined and notified
Proposed date of entry into force: To be determined

	10.
	Provision of comments
Final date for comments: 20 January 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Contact person(s):
Ms. Bahati Samillani (NEP officer) and Mr. Clavery Chausi
Tanzania Bureau of Standards (TBS)
Morogoro/Sam Nujoma Road, Ubungo
P O Box 9524
Dar Es Salaam
Tel: +(255) 22 2450206
Email: nep@tbs.go.tz; bahati.samillani@tbs.go.tz
Website: http://www.tbs.go.tz
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