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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: JORDAN
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Jordan Standards and Metrology Organization (JSMO)
Tel: +962 6 5301225, Fax: +962 6 5301249
E-mail: jsmo@jsmo.gov.jo
Website: http://www.jsmo.gov.jo/

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Ferrous metals (ICS code(s): 77.080)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): Standard specification for deformed and plain carbon steel bars for
concrete reinforcement; (15 page(s), in Arabic)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://jsmo.gov.jo/EBV4.0/Root_Storage/AR/EB_UsefullLinks/DJS-2126-2025.pdf

	6.
	Description of content: This Technical Regulation specifies the mandatory requirements for deformed and plain carbon steel bars used for concrete reinforcement, whether supplied as straight cut lengths or in coils. It covers requirements related to materials and manufacturing, chemical composition, transverse rib geometry and measurements, and mechanical properties including yield strength, tensile strength, elongation, and bending. The regulation also defines dimensional requirements, mass per unit length and permissible tolerances, as well as provisions for testing, sampling, number of tests and retesting, inspection procedures, rejection and appeal, marking, and labelling. This document aims to ensure the quality, safety, and fitness for use of carbon steel reinforcing bars in concrete structures.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of human health or safety

	8.
	Relevant documents: 
· International Standard ISO 6935-1:2007, Steel for the reinforcement of concrete — Part 1: Plain bars.
· International Standard ISO 6935-2:2019, Steel for the reinforcement of concrete — Part 2: Ribbed bars.
· ASTM A615/A615M-24, Standard Specification for Deformed and Plain Carbon-Steel Bars for Concrete Reinforcement.
· Jordanian Standard JS 119:2022, Labeling — Industrial Products Labeling

	9.
	Proposed date of adoption: 18 February 2026
Proposed date of entry into force: 18 May 2026

	10.
	Provision of comments
Final date for comments: 20 February 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Jordan Standards and Metrology Organization (JSMO)
WTO/TBT Enquiry Point
Tel: +962 6 5301225
Fax: +962 6 5301249
E-mail: enquiry@jsmo.gov.jo
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