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NOTIFICATION
Addendum
The following communication, dated 15 January 2026, is being circulated at the request of the delegation of the United States of America.

_______________


Title: Federal Motor Vehicle Safety Standards: Anti-Ejection Glazing for Bus Portals; Mandatory Applicability Beginning 30 October 2027

	[bookmark: _Hlk24973414]Reason for Addendum:

	[ ]
	Comment period changed - date: 

	[ ]
	Notified measure adopted - date: 

	[ ]
	Notified measure published - date: 

	[X]
	Notified measure enters into force - date: 15 January 2026; this final rule is effective 15 January 2026. The compliance date of this final rule is 30 October 2027. Optional early compliance is permitted. If you wish to petition for reconsideration of this rule, your petition must be received by 2 March 2026.

	[X]
	[bookmark: _Ref40866877]Text of final measure available from[footnoteRef:2]:  [2:  This information can be provided by including a website address, a pdf attachment, or other information on where the text of the final/modified measure and/or interpretive guidance can be obtained.] 

https://members.wto.org/crnattachments/2026/TBT/USA/final_measure/26_00359_00_e.pdf

	[ ]
	Notified measure withdrawn or revoked - date: 
Relevant symbol if measure re-notified: 

	[ ]
	Content or scope of notified measure changed and text available from1: 
New deadline for comments (if applicable): 

	[ ]
	Interpretive guidance issued and text available from1: 

	[ ]
	Other: 



Description: This document partially grants a petition for reconsideration of the 30 October 2024 final rule (notified as G/TBT/N/USA/1123/Add.1) that established Federal Motor Vehicle Safety Standard (FMVSS) No. 217a, ''Anti-ejection glazing for bus portals; Mandatory applicability beginning 30 October 2027.'' The standard intends to drive installation of advanced glazing in over-the- road buses (motorcoaches) and other large buses to reduce occupant ejections. This final rule revises the minimum size requirement for applicable portals, adds a figure to illustrate a daylight opening periphery, and clarifies the target location for edge impact tests. This document denies all other portions of the petition for reconsideration, including revising the definition of ''daylight opening.''
Effective Date: This final rule is effective 15 January 2026.
Compliance Date: The compliance date of this final rule is 30 October 2027. Optional early compliance is permitted.
Petitions for Reconsideration: If you wish to petition for reconsideration of this rule, your petition must be received by 2 March 2026.
91 Federal Register (FR) 1709, 15 January 2026; Title 49 Code of Federal Regulations (CFR) Part 571:
https://www.govinfo.gov/content/pkg/FR-2026-01-15/html/2026-00728.htm
https://www.govinfo.gov/content/pkg/FR-2026-01-15/pdf/2026-00728.pdf
This final rule; partial grant of a petition for reconsideration is identified by Docket Number NHTSA-2026-0001. The Docket Folder is available on Regulations.gov at https://www.regulations.gov/docket/NHTSA-2026-0001/document. The Docket provides access to primary document and comments if received, which is also accessible from Regulations.gov by searching the Docket Number. WTO Members and their stakeholders are asked to submit petitions for reconsideration of this rule to the USA TBT Enquiry Point by or before 4pm Eastern Time on 2 March 2026. Petitions for reconsideration received by the USA TBT Enquiry Point from WTO Members and their stakeholders will be shared with NHTSA and will be submitted on Regulations.gov if received within the comment period.
Previous actions notified under the symbol G/TBT/N/USA/1123 are identified by Docket Numbers NHTSA-2016-0052 and NHTSA-2024-0061.
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