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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: THE SEPARATE CUSTOMS TERRITORY OF TAIWAN, PENGHU, KINMEN AND MATSU
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Bureau of Standards, Metrology and Inspection (BSMI)
Ministry of Economic Affairs

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [X], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Portland cement (excl. white, whether or not artificially coloured) (HS code(s): 252329); Cement, whether or not coloured (excl. portland cement and aluminous cement) (HS code(s): 252390)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): Proposal for Amendments to the Legal Inspection Requirements for Cement; (1 page(s), in Chinese), (2 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/TPKM/26_01127_00_x.pdf
https://members.wto.org/crnattachments/2026/TBT/TPKM/26_01127_00_e.pdf
WTO TBT Enquiry Point, Email: tbtenq@bsmi.gov.tw

	6.
	Description of content: With a view to enhancing the quality of cements, the Bureau of Standards, Metrology and Inspection (BSMI) proposes to adopt the updated version of CNS 61, Portland cements, published in 2025, as the inspection standard. 
The main change of CNS 61 is that the maximum limit for chloride ion content in type I/IA Portland cement is revised from 240 ppm to 350 ppm, and the requirement of chloride ion content is modified from an optional chemical composition provision to a mandatory chemical composition standard requirement (i.e., reclassified as a CNS 61 quality item).
The conformity assessment procedures remain the same, i.e., Monitoring Inspection (MI) or Monitoring Inspection of Products from Premises with Registered Management System (MS-Based Monitoring Inspection).

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Prevention of deceptive practices and consumer protection; Quality requirements

	8.
	Relevant documents: 
Government Gazette, Vol. 032, No. 033, dated 24 February 2026
(https://gazette.nat.gov.tw/egFront/e_detail.do?metaid=163778)
The Commodity Inspection Act
Relevant notifications:
· G/TBT/N/TPKM/505

	9.
	Proposed date of adoption: 1 July 2026
Proposed date of entry into force: 1 July 2026

	10.
	Provision of comments
Final date for comments: 26 April 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
WTO TBT Enquiry Point
Bureau of Standards, Metrology and Inspection
Ministry of Economic Affairs
No. 4, Sec. 1, Jinan Rd., Zhongzheng Dist.
Taipei City 100, Taiwan
Tel: +(886-2) 23431700#1566
Fax: +(886-2) 23431804
Email: tbtenq@bsmi.gov.tw
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