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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: UNITED STATES OF AMERICA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
National Highway Traffic Safety Administration (NHTSA), U.S. Department of Transportation (DOT) [2298]

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Automated driving systems (ADS) equipped vehicles; Transmissions, suspensions (ICS code(s): 43.040.50)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): Federal Motor Vehicle Safety Standards; Modernization of FMVSS No. 102 To Accommodate ADS-Equipped Vehicles; (6 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/USA/26_01496_00_e.pdf

	6.
	Description of content: Notice of proposed rulemaking - The National Highway Traffic Safety Administration (NHTSA) is proposing to amend Federal Motor Vehicle Safety Standard (FMVSS) No. 102, "Transmission shift position sequence, starter interlock, and transmission braking effect.'' The proposed modification would except vehicles equipped with Automated Driving Systems (ADS) that do not have manually operated driving controls from the requirement for a transmission shift position display. This rulemaking would remove unnecessary regulatory burdens and costs associated with a display designed to aid a person driving the vehicle. As the transmission shift position display does not fulfill the same safety need in an ADS-equipped vehicle without manually operated driving controls, the amendment will not impact vehicle safety. This action is part of a larger NHTSA effort to address vehicle automation in the agency's regulations.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Cost saving and productivity enhancement

	8.
	Relevant documents: 
91 Federal Register (FR) 12532, 16 March 2026; Title 49 Code of Federal Regulations (CFR) Part 571:
https://www.govinfo.gov/content/pkg/FR-2026-03-16/html/2026-05024.htm
https://www.govinfo.gov/content/pkg/FR-2026-03-16/pdf/2026-05024.pdf
This notice of proposed rulemaking is identified by Docket Number NHTSA-2026-0628. The Docket Folder is available on Regulations.gov at https://www.regulations.gov/docket/NHTSA-2026-0628/document and provides access to primary documents as well as comments received. Documents are also accessible from Regulations.gov by searching the Docket Number.
Relevant notifications:
· G/TBT/N/USA/1487
· G/TBT/N/USA/1487/Add.1
· G/TBT/N/USA/1593
· G/TBT/N/USA/1593/Add.1
· G/TBT/N/USA/1675
· G/TBT/N/USA/1675/Add.1

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: To be determined

	10.
	Provision of comments
Final date for comments: 15 April 2026
[ ] 60 days from notification 
WTO Members and their stakeholders are asked to submit comments to the USA TBT Enquiry Point by or before 4pm Eastern Time on 15 April 2026. Comments received by the USA TBT Enquiry Point from WTO Members and their stakeholders will be shared with NHTSA and will also be submitted to the Docket on Regulations.gov if received within the comment period.
Contact details of agency or authority designated to handle comments regarding the notification: 
Please submit comments to: USA WTO TBT Enquiry Point, Email: usatbtep@nist.gov
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