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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: CHINA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
State Administration for Market Regulation (Standardization Administration of the P.R.C.)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Arcing fault detector (HS code(s): 903180); (ICS code(s): 13.220.20)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): National Standard of the P.R.C., Electrical fire monitoring system—Part4: Arcing fault detector; (31 page(s), in Chinese)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/CHN/26_01644_00_x.pdf

	6.
	Description of content: This document specifies the terms and definitions of arcing fault detector, stipulates the tests, inspection rules, marking and instruction manuals and describes the corresponding test methods.
This document applies to AC arcing fault detector installed and used in electrical circuits not exceeding 15kW in industrial and civil buildings, as well as DC arcing fault detector with a maximum open circuit voltage not exceeding 1500V DC. Arcing fault detector used for electrical fire monitoring in other devices, as well as arcing fault detector with special requirements in other environments, are also applicable to this document, except where special requirements are otherwise specified by relevant standards.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of human health or safety

	8.
	Relevant documents: 
-

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 12 months after standard approval

	10.
	Provision of comments
Final date for comments: 23 May 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
WTO/TBT National Notification and Enquiry Center of the People's Republic of China
Tel：+86 10 57954633/ 57954627
E_mail: tbt@customs.gov.cn
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