	[bookmark: bmkRestricted]
	

	[image: ]
	

	
	[bookmark: bmkSymbols]G/TBT/N/CHN/2296

	
	[bookmark: spsDateDistribution][bookmark: bmkDate]13 July 2026

	[bookmark: bmkSerial](26-5002)
	[bookmark: bmkTotPages]Page: 1/2

	[bookmark: bmkCommittee]Committee on Technical Barriers to Trade
	[bookmark: bmkLanguage][bookmark: spsOriginalLanguage]Original: English



tbtSymbol

- 1 -

[bookmark: spsSymbolHeader]G/TBT/N/CHN/2296

- 2 -

NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: CHINA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
State Administration for Market Regulation (Standardization Administration of the P.R.C.)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): LED flat panel luminaires (HS code(s): 940542); (ICS code(s): 27.010)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): National Standards of the P.R.C., Minimum allowable values of energy efficiency and energy efficiency grades of LED flat panel luminaires; (6 page(s), in Chinese)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/CHN/26_03587_00_x.pdf

	6.
	Description of content: This document specifies the energy efficiency grades, minimum allowable values of energy efficiency, test methods and implementation date of this standard for LED flat panel luminaires.
This document applies to LED flat panel luminaires with LED light sources, a rated voltage of AC 250V and a rated frequency of 50 Hz (including LED light sources and control gears). The thickness of LED flat panel luminaire shell not exceed 85mm, excluding its external controlgear(s).
This document does not apply to LED flat panel luminaires with additional non-lighting power-consuming functions, with colorful light or those whose rated correlated color temperatures below 2700 K or above 6500 K, or with colors/patterns/ decorations on the continuous luminous surfaces.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of the environment; Quality requirements

	8.
	Relevant documents: 
-

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: To be determined

	10.
	Provision of comments
Final date for comments: 11 September 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
WTO/TBT National Notification and Enquiry Center of the People's Republic of China
Tel：+86 10 57954633/ 57954642
E_mail: tbt@customs.gov.cn
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