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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: CHINA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
State Administration for Market Regulation (Standardization Administration of the P.R.C.)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Materials for building thermal insulation, polyurethane polyether blend, sprayed rigid polyurethane foam (HS code(s): 390729); (ICS code(s): 83.080)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): National Standard of the P.R.C, Requirement of flame resistance for spray-applied rigid foam polyurethane blended polyol and products used in building thermal insulation materials; (11 page(s), in Chinese)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/CHN/26_04155_00_x.pdf

	6.
	Description of content: This document specifies requirements, test methods, judgment rules, accompanying documents, packaging marking, and application requirements related to the flame-retardant properties of polyol blends and their products used for sprayed rigid polyurethane foam thermal insulation in buildings. 
This document applies only to polyol blends and their products for sprayed rigid polyurethane foam used in wall, roof, and floor insulation for buildings (including cold storage facilities), and does not cover those used for insulation of tanks and pipelines.
This document applies to quality management and control by both manufacturers and users of sprayed rigid polyurethane foam polyol blends, as well as to acceptance inspection and testing by relevant parties.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Prevention of deceptive practices and consumer protection; Protection of human health or safety; Quality requirements

	8.
	Relevant documents: 
-

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 12 months after approval

	10.
	Provision of comments
Final date for comments: 9 October 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
WTO/TBT National Notification and Enquiry Center of the People's Republic of China
Tel：+86 10 57954633/ 57954642
E_mail: tbt@customs.gov.cn
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