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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: CHINA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
State Administration for Market Regulation (Standardization Administration of the P.R.C.)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Fans (HS code(s): 8504); (ICS code(s): 27.010)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): National Standard of the P.R.C., Minimum allowable values of energy efficiency and energy efficiency grades for fan; (9 page(s), in Chinese)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/CHN/26_04310_00_x.pdf

	6.
	Description of content: This document specifies the energy efficiency grades, energy efficiency limit values, and test methods for fans.
This document applies to general-purpose centrifugal fans (including backward centrifugal fans, forward-curved centrifugal fans, radial centrifugal fans, volute-free centrifugal fans, and low characteristic speed centrifugal fans) with motor input power ranging from 0.125 kW to 500 kW, general-purpose axial fans and reversible axial fans, mixed-flow fans, fire smoke exhaust fans, and non-metallic material corrosion-resistant fans.
This document applies to products that are produced in series or specially designed and manufactured, including fans with impellers mounted on the fan shaft, excluding driving devices, additional devices, or accessories, as well as fans with impellers mounted on or connected to electric motors, equiped with or without driving devices, casings, and variable speed drive devices.
This document does not apply to ventilators, explosion-proof ventilators, box fans, roof ventilators, and air curtain machines used in motor vehicles, trains, and aircraft, as well as jet fans used for ventilation in parking lots and tunnels.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of the environment; Cost saving and productivity enhancement

	8.
	Relevant documents: 
-

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: 12 months after approval

	10.
	Provision of comments
Final date for comments: 18 October 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
WTO/TBT National Notification and Enquiry Center of the People's Republic of China
Tel：+86 10 57954633/ 57954642
E_mail: tbt@customs.gov.cn
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