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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: THE STATE OF KUWAIT
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Public Authority for Industry
Standard and Metrology Department (KOWSMD)

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): All products fall under scope of " Controlgear for electric light sources – Safety – Part 2-13: Particular requirements – Electronic controlgear for LED light sources " 

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): Controlgear for electric light sources – Safety – Part 2-13: Particular requirements – Electronic controlgear for LED light sources; (19 page(s), in English), (19 page(s), in French)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/KWT/26_05241_00_e.pdf

	6.
	Description of content: This part of IEC 61347 specifies safety requirements for electronic controlgear for LED light sources for use on DC supplies up to 1 500 V or on AC supplies up to 1 000 V at 50 Hz or 60 Hz.
This document is applicable for electronic controlgear for LED light sources with an output voltage (RMS) not higher than 1 000 V.
NOTE 1 Control units, such as devices connected between the power supply unit and LED light sources that control or adjust the operation of LED light sources, are covered by this document.
NOTE 2 Performance requirements are covered by IEC 62384.
NOTE 3 Such controlgear can also be used for electric sources producing optical radiation with the same technology used for purposes different than illumination and producing radiation other than visible spectrum.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Protection of human health or safety

	8.
	Relevant documents: 
GSO IEC 61347-2-13:2025 (Controlgear for electric light sources - Safety - Part 2-13: Particular requirements - Electronic controlgear for LED light sources)

	9.
	Proposed date of adoption: 30 days from final date for comments.
Proposed date of entry into force: 1 year from adoption.

	10.
	Provision of comments
Final date for comments: 6 December 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Public Authority for Industry
P.O.Box 4690, Safat
13047 Kuwait
Tel: (+965) 25302622
E-mail: Enquiry_point@pai.gov.kw
Website: http://www.pai.gov.kw
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