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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: UGANDA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Uganda National Bureau of Standards
Plot 2-12 ByPass Link, Bweyogerere Industrial and Business Park
P.O. Box 6329
Kampala, Uganda
Tel: +(256) 4 1733 3250/1/2
Fax: +(256) 4 1428 6123
E-mail: info@unbs.go.ug
Website: https://www.unbs.go.ug

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Wood pellets (HS code(s): 440131); Solid fuels (ICS code(s): 75.160.10); Non-carbonised pellets

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): DUS 2558:2026, Solid biofuel — Non-carbonised pellets — Specifications, First edition; (16 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/UGA/26_05376_00_e.pdf

	6.
	Description of content: This Draft Uganda Standard specifies requirements and test methods for produced pellets that are derived from forest residues, woody biomass, wood processing residues, recycled wood, herbaceous biomass, fruit biomass, aquatic biomass, agro-industrial residues, faecal sludge and organic waste. This standard does not apply to pellets made from torrefied biomass materials.

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Consumer information, labelling; Prevention of deceptive practices and consumer protection; Protection of human health or safety; Protection of the environment; Quality requirements; Harmonization; Reducing trade barriers and facilitating trade; Cost saving and productivity enhancement

	8.
	Relevant documents: 
1. ISO 3310-2, Test sieves ― Technical requirements and testing ― Part 2: Test sieves of perforated metal plate.
2. ISO 16559, Solid biofuels — Terminology, definitions and descriptions
3. ISO 17225-7, Solid biofuels — Fuel specifications and classes — Part 7: Graded non-woody briquettes
4. ISO 18134-2, Solid biofuels — Determination of moisture content — Part 2: Simplified method
5. ISO 17225-1, Solid biofuels — Fuel specifications and classes — Part 1: General requirements
6. ISO 18122. Solid biofuels — Determination of ash content
7. ISO 18125, Solid biofuels — Determination of calorific value
8. ISO 17828; Solid biofuels — Determination of bulk density
9. ISO 17831-1; Solid biofuels — Determination of mechanical durability of pellets and briquettes — Part 1: Pellets
10. ISO 16948; Solid biofuels — Determination of total content of carbon, hydrogen and nitrogen
11. ISO 16994; Solid biofuels and pyrogenic biocarbon — Determination of sulfur and chlorine content
12. ISO 5370; Solid biofuels — Determination of fines content in pellets,
13. ENplus ST 1001:2022, wood pellets – Requirements for companies, second edition

	9.
	Proposed date of adoption: To be determined
Proposed date of entry into force: To be determined

	10.
	Provision of comments
Final date for comments: 13 December 2026
[X] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Uganda National Bureau of Standards
Plot 2-12 ByPass Link, Bweyogerere Industrial and Business Park
P.O. Box 6329
Kampala, Uganda
Tel: +(256) 4 1733 3250/1/2
Fax: +(256) 4 1428 6123
E-mail: info@unbs.go.ug
Website: https://www.unbs.go.ug
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