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NOTIFICATION
The following notification is being circulated in accordance with Article 10.6

	1.
	Notifying Member: BURUNDI, KENYA, RWANDA, TANZANIA, UGANDA
If applicable, name of local government involved (Articles 3.2 and 7.2): 

	2.
	Agency responsible: 
Kenya Bureau of Standards

	3.
	Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [X], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], Other: 

	4.
	Products covered (HS codes or national tariff lines. ICS numbers may be provided in addition, where applicable): Pressure vessels (ICS code(s): 23.020.30)

	5.
	Details of notified document(s) (title, number of pages and languages, means of access): DEAS 1377: 2026 Liquefied petroleum gas storage installations — Domestic, commercial and industrial and reticulation systems; (20 page(s), in English)
Link to notified document(s) and/or contact details for agency or authority which can provide copies upon request: 
https://members.wto.org/crnattachments/2026/TBT/KEN/26_05445_00_e.pdf
Kenya Bureau of Standards
P.O. Box: 54974-00200, Nairobi, Kenya
Telephone: + (254) 020 605490, 605506/6948258
Fax: + (254) 020 609660/609665
E-mail: info@kebs.go.ke; Website: http://www.kebs.go.ke

	6.
	Description of content: This daft East African Standard specifies requirements for the design, installation, testing, commissioning, operation, inspection and maintenance of LPG reticulation systems serving domestic, commercial and industrial consumer installations supplied from bulk LPG storage vessels. 
This standard does not cover LPG storage installations at:
1. Refineries and cylinder/ container filling plants;
2. LPG-air (Synthetic natural gas) distribution plants;
3. Aerosol plants; and
4. Auto LPG stations

	7.
	Objective and rationale, including the nature of urgent problems where applicable: Quality requirements; Harmonization

	8.
	Relevant documents: 
1. ASME, Code for boilers and pressure storage vessels – Section VIII, Divisions I and II
2. EN 13445; Unfired pressure vessels
3. EAS 1105, Liquefied petroleum gas - specification.
4. EAS 924-2; Handling, storage, and distribution of Liquefied Petroleum Gas (LPG) in domestic, commercial, and industrial installations — Code of practice Part 2:LPG installations involving gas storage vessels of individual water capacity exceeding 150 L and combined water capacity not exceeding 9000 L per installation
5. EAS 924-3; Handling, storage and distribution of Liquefied Petroleum Gas (LPG) in domestic, commercial, and industrial installations — Code of practice — Part 3: LPG installations involving storage vessels of individual water capacity exceeding 9 000 L
6. ISO 2928, Rubber hoses and hose assemblies for liquefied petroleum gas (LPG) in the liquid or gaseous phase and natural gas up to 2,5 MPa (25 bar) — Specification
7. ISO 4437-1, Plastics piping systems for the supply of gaseous fuels — Polyethylene (PE) Part 1: General
8. NFPA 58, LP-Gas Code Handbook

	9.
	Proposed date of adoption: 31 March 2027
Proposed date of entry into force: To be determined

	10.
	Provision of comments
Final date for comments: 20 December 2026
[ ] 60 days from notification 
Contact details of agency or authority designated to handle comments regarding the notification: 
Kenya Bureau of Standards
WTO/TBT National Enquiry Point
P.O. Box: 54974-00200, Nairobi, Kenya
Telephone: + (254) 020 605490, 605506/6948258
Fax: + (254) 020 609660/609665
E-mail: E-mail: info@kebs.go.ke; Website: http://www.kebs.go.ke
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